Configuration	YS-F1Pro
STM32CubeMX 	4.14.0
Date	05/07/2016
MCU	STM32F103ZETx



PERIPHERALS	MODES	FUNCTIONS	PINS
RCC	Crystal/Ceramic Resonator	RCC_OSC_IN	OSC_IN
RCC	Crystal/Ceramic Resonator	RCC_OSC_OUT	OSC_OUT
SYS	SysTick	SYS_VS_Systick	VP_SYS_VS_Systick
USART1	Asynchronous	USART1_RX	PA10
USART1	Asynchronous	USART1_TX	PA9



Pin Nb	PINs	FUNCTIONs	LABELs
23	OSC_IN	RCC_OSC_IN	
24	OSC_OUT	RCC_OSC_OUT	
101	PA9	USART1_TX	
102	PA10	USART1_RX	



SOFTWARE PROJECT

Project Settings : 
Project Name : YS-F1Pro
Project Folder : E:\硬石电子\2. 软件设计(HAL库版本)\1. 软件设计之基本裸机例程(HAL库版本)\YSF1_HAL-008. USART-调试串口
Toolchain / IDE : MDK-ARM V5
Firmware Package Name and Version : STM32Cube FW_F1 V1.3.1


Code Generation Settings : 
STM32Cube Firmware Library Package : Copy all used libraries into the project folder
Generate peripheral initialization as a pair of '.c/.h' files per IP : Yes
Backup previously generated files when re-generating : No
Delete previously generated files when not re-generated : Yes
Set all free pins as analog (to optimize the power consumption) : No


Toolchains Settings : 
Compiler Optimizations : Balanced Size/Speed






